How to install and configure Kenkey evat monitoring tool

1.install kenkey and allow it to create shortcut on desktop
2.right click on kenkey shortcut and go to open file location
3. within that folder , locate CONFIG_FILE_1.txt
4. open file to edit , and put one till IP by replacing loopback ip(127.0.0.1) on line 2.
5.if tomcat service port is not default one, put your dedicated port on line 5 by replacing 8080.
6. save the file.
7. the kenkey installation location shall have read & write permissions for kenkey to run well.
8.check the file colled 'Urutambi.txt' and edit it accordingly